SOUND/LIGHTS/STAGE: PURCHASER shall provide adequate sound/light production for size of venue.  
PURCHASER will provide a sound technician at load-in to assist our crew and engineer with wiring your stage and assist with any questions the may have with the house system. PURCHASER shall provide a complete lighting system and technician for a professional appearance of the stage and show. All sound and lighting technicians MUST be present at sound check.
Stage
   Stage will be a minimum of 32' x 24'   with a 12 -18" tall  8'x8' drum riser, center stage at the rearmost allowable position.  Also the will be a 12" tall riser , stage left with a minimum area of 8'x6' for the back up singers.
   If agreed upon by Second Helping, or their agent,  a smaller stage may be used ,but  there must be 2(two) outboard platforms for PA and/or trusses that will not encroach on the main stage.
Any and all outdoor stages must have rain/sun protection covering the band and it's equipment.  Stage will have steps/ and or ramps if over 12" from the loading height.   Access must be allowed for Second Helping's equipment vehicle and trailer to the stage area and parking in the area.

Electricity
Second Helping requires a minimum of 4 20 amp circuits, not including and PA or lighting.  Power is to be supplied to the designated stage areas.
   In the event of a generator being used,  surge protection/ power conditioning must be provided, and the generator must have a fuel run time of a minimum of 8 hours.  No food services or non-stage lighting will be run from said generator.  Unwanted hums and buzzing will affect the quality of the show.
   Lighting will be provided during set up/ breakdown until completion of load out.